|  |
| --- |
| White Spirit – high FBP |
| Properties | Unit | Specification | Test Method |
| Color | Saybolt | 24 | ASTM D 156 |
| Flash Point | vol% | 45 | ASTM D 93 |
| Aromatic | Wt% | 32.20 | ASTM D 5580 |
| Sulfur Total | g/cm3 | 0.0828 | ASTM D 4294 |
| Density @ 15 **°**C | **°**C | 0.795 | ASTM D 1298 |
| IBP | **°**C | 155 | ASTM D 86 |
| 10% Evaporated | **°**C | 162 |
| 20% Evaporated | **°**C | 165 |
| 30% Evaporated | **°**C | 168 |
| 40% Evaporated | **°**C | 171 |
| 50% Evaporated | **°**C | 174 |
| 60% Evaporated | **°**C | 179 |
| 70% Evaporated | **°**C | 183 |
| 80% Evaporated | **°**C | 193 |
| 90% Evaporated | **°**C | 209 |
|  |  |  |
| 95% Evaporated | RDR Logo Vertical**°**C | 223 |
| 100% Evaporated | **°**C | - |
| FBP | **°**C | 245 |
| Cetane | - | - | ASTM D 976 |